Demo List Information
|--AC_AM
|    :Demo how to use the AccCode and AccMask in the CAN 2.0A specification.
|--DUAL_F
|    :Demo how to use the AccCode and AccMask to set dual filter in the CAN 2.0A specification.
|--All_Demo
|    :Demo the total functions provided by the XC100L.lib.
|--L1_L2_L3
|    :Demo how to use the L1, L2, and L3 LEDs.
|--RxInt
|    :Demo how to receive the CAN 2.0A messages by interrupt mode.
|--RxPoll
|    :Demo how to receive the CAN 2.0A messages by polling mode.
|--SearchCANBaud
|    :Demo how to scan the CAN baudrate.
|--TxInt
|    :Demo how to send the CAN 2.0A messages to the CAN network by interrupt mode.
|--TxPoll
|    :Demo how to send the CAN 2.0A messages to the CAN network by polling mode.
|--UserInt
|    :Demo how to use the UserCANInt function to apply the users' CAN interrupt service routine.
|--SCH_Baud
|    :Demo how to search the necessary CAN bus baud rate.