; install information file for DIO-64 Series Card

[Version]
Signature="$Windows NT$"
Class=DAQCard
ClassGuid={337B6A7D-6400-4a90-AF29-9924EE97532F}
Provider=%Company%
DriverVer=12/15/2000,1.2.01.0

[ClassInstall32]
AddReg=DAQCardClassAddReg

[DAQCardClassAddReg]
HKR,,,,"DAQCard"
HKR,,Icon,,-5

[Manufacturer]
%Company% = SECTION_0

[SECTION_0]
%Product%=Drv.Install


[DestinationDirs]
Drv.Files.Driver=10,System32\Drivers
Drv.Files.Driver.NTx86=10,System32\Drivers

[SourceDisksNames]
1="NAPDIO build directory",,,

[SourceDisksFiles]
NAPDIO.sys=1

[SourceDisksFiles.x86]
NAPDIO.sys=1

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 98

[Drv.Install]
CopyFiles=Drv.Files.Driver
AddReg=Drv.AddReg
LogConfig=Drv.LConfig01, Drv.LConfig02

[Drv.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,NAPDIO.sys

[Drv.Files.Driver]
NAPDIO.sys

[Drv.LConfig01]
ConfigPriority=DESIRED
IOConfig=2A0-2AF,2B0-2BF,\
         2C0-2CF,2D0-2DF,2E0-2EF,2F0-2FF,\
         300-30F,310-31F,320-32F,330-33F,\
         340-34F,350-35F,360-36F,370-37F,\
         380-38F,390-39F,3A0-3AF,3B0-3BF,\
         3C0-3CF,3D0-3DF,3E0-3EF,3F0-3FF,\
         200-20F,210-21F,220-22F,230-23F,\
         240-24F,250-25F,260-26F,270-27F,\
         280-28F,290-29F
IRQConfig=15,12,11,10,9,7,5,4,3

[Drv.LConfig02]
ConfigPriority=NORMAL
IOConfig=2A0-2AF,2B0-2BF,\
         2C0-2CF,2D0-2DF,2E0-2EF,2F0-2FF,\
         300-30F,310-31F,320-32F,330-33F,\
         340-34F,350-35F,360-36F,370-37F,\
         380-38F,390-39F,3A0-3AF,3B0-3BF,\
         3C0-3CF,3D0-3DF,3E0-3EF,3F0-3FF,\
         200-20F,210-21F,220-22F,230-23F,\
         240-24F,250-25F,260-26F,270-27F,\
         280-28F,290-29F

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Windows 2000

[Drv.Install.NTx86]
CopyFiles=Drv.Files.Driver.NTx86
LogConfig=Drv.LConfig01, Drv.LConfig02

[Drv.Files.Driver.NTx86]
NAPDIO.sys,,,%COPYFLG_NOSKIP%

[Drv.Install.NTx86.Services]
AddService = NAPDIO, %SPSVCINST_ASSOCSERVICE%, Drv.Service

[Drv.Service]
DisplayName    = %Drv.ServiceName%
ServiceType    = 1
StartType      = 2
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %10%\System32\Drivers\NAPDIO.sys

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
; Strings

[Strings]
Company="ICPDAS Co. LTD"
Product="ICPDAS DIO-64 Digital I/O Card"
Drv.ServiceName="ICPDAS NAPDIO Driver"

SPSVCINST_ASSOCSERVICE=0x00000002	; Driver service is associated with device being installed
COPYFLG_NOSKIP=2	; Do not allow user to skip file
SERVICE_KERNEL_DRIVER=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1
