/**************************************************************/
/*                                                            */
/*  A-626/A-628 for DOS User                                  */
/*                                                            */
/*  version : 2.0                                             */
/*  Update  : Mar-12, 1999                                    */
/*                                                            */
/**************************************************************/

The READNE.TXT contains the newset information for A626/A628.
Please reading this file before install.

The contents in this disk are valid for A626/A628 .
The directories as follows:

	|-\[A626]
        |     |
        |     |-\[Cal]          <-- Calibration program for A626
        |     |
        |     |-\[Demo]
        |         |-\[TC2]     	<-- Turbo C 2.0 Demo program
        |         |   |-Demo1       <-- UniPolar5V, DA demo
        |         |   |-Demo2       <-- DI/DO demo
        |         |
        |         |-\[MSC6]    	<-- Microsoft C 6.0 Demo program
        |         |   |-Demo1       <-- UniPolar5V, DA demo
        |         |   |-Demo2       <-- DI/DO demo
        |         |
	|         |-\[BC31]	<-- Borland C++ 3.1 Demo program
        |         |   |-Demo1       <-- UniPolar5V, DA demo
        |         |   |-Demo2       <-- DI/DO demo
        |         |
        |         |-\[QBasic]   <-- Quick Basic demo program
        |             |-Demo1       <-- Unipolar mode 0-5V , DA demo
        |             |-Demo2       <-- Bipolar mode +/-5V , DA demo
        |             |-Demo3       <-- Uipolar mode  0-10V, DA demo
        |             |-Demo4       <-- Uipolar mode +/-10V, DA demo
	|
	|-\[A628]
        |     |
        |     |-\[Cal]          <-- Calibration program for A628
        |     |
	|     |-\[DEMO]
        |         |-\[TC2]     	<-- Turbo C 2.0 Demo program
        |         |   |-Demo1       <-- UniPolar5V, DA demo
        |         |   |-Demo2       <-- DI/DO demo
        |         |
        |         |-\[MSC6]    	<-- Microsoft C 6.0 Demo program
        |         |   |-Demo1       <-- UniPolar5V, DA demo
        |         |   |-Demo2       <-- DI/DO demo
        |         |
	|         |-\[BC31]	<-- Borland C++ 3.1 Demo program
        |         |   |-Demo1       <-- UniPolar5V, DA demo
        |         |   |-Demo2       <-- DI/DO demo
        |         |
        |         |-\[QBasic]   <-- Quick Basic demo program
        |             |-Demo1       <-- Unipolar mode 0-5V , DA demo
        |             |-Demo2       <-- Bipolar mode +/-5V , DA demo
        |             |-Demo3       <-- Uipolar mode  0-10V, DA demo
        |             |-Demo4       <-- Uipolar mode +/-10V, DA demo
	|
	|-\[Lib]
        |     |-A628s.Lib   	<-- Small   Model Library
        |     |-A628m.Lib   	<-- Medium  Model Library
        |     |-A628c.Lib   	<-- Compact Model Library
        |     |-A628l.Lib   	<-- Large   Model Library
        |     |-A628h.Lib   	<-- Huge    Model Library
        |     |
        |     |-A628.h          <-- Header file for A626/A628
        |     |-A628u.c         <-- Folating point functions for A626/A628
        |
	|-\[LibSrc]             <-- Library source code for BC++31
	|
	|-Readme.Txt		<-- this file



********************
***    Errata:   ***
********************

A626/A628 Hardware manual 

  *****************************
  Page 13: 2.6. Pin Assignment
     Error...
        Pin.27: A.GND
        Pin.36: A.GND
     Correct...
        Pin.27: Not used
        Pin.36: Not used


  *************************************
  Page 17: 3.1.1. A626 I/O Port Address
     Error...
        Address:          Function:        Read/Write:
        ***************   ***************  ******************
        Base + 0xC        D/I/O Bit 0-7    Write/Read
        Base + 0xD        D/I/O Bit 8-15   Write/Read
     Correct...
        Address:          Function:        Read/Write:
        ***************   ***************  ******************
        Base + 0xC        D/O Bit 8-15     Write
        Base + 0xD        D/O Bit 0-7      Write
        Base + 0xE        D/I Bit 8-15     Read
        Base + 0xF        D/I Bit 0-7      Read


   


 		