<< Web HMI Demo 7 , please download "wphmi_07" project to WinPAC >>
AIO demo (slot 2: I-87024W, 3: 8017HW, please wire AI Ch1 to AO CH1, CH2 to CH2)
AIO's scaling action of this demo is done in the Browser of PC.
Please refer to Web HMI demo 6 for scaling action done in the ISaGRAF program.

Communication state = 0
Analog Input 1 at Modbus No. 1 = A1
Analog Input 2 at Modbus No. 2 = A2
Analog Output 1 at Modbus No. 3 = A3
Analog Output 2 at Modbus No. 4 = A4

Please enter Analog output 2, unit is Volt