<< Web HMI Demo 6 , please download "vphmi_06" project to ViewPAC >>
AIO demo (slot 1: I-87024W, 2: 8017HW, please wire AI Ch1 to AO CH1, CH2 to CH2)
AIO's scaling action of this demo is done in the ISaGRAF program.
Please refer to Web HMI demo 7 for scaling action done in the browser of PC.

Communication state = 0
Analog Input 1 at Modbus No. 1 = F1
Analog Input 2 at Modbus No. 3 = F3
Analog Output 1 at Modbus No. 11 = F11
Analog Output 2 at Modbus No. 13 = F13

Please enter Analog output 2, unit is Volt