ViewPAC Web HMI Demo 13 :

Rcord 4-Ch Voltage in a RAM Space and then save to "\Web_Data1\curve1.js" file in ViewPAC .

Then PC can download it and use M.S. Excel to draw a Trend Curve.

Note:

1. Please download ISaGRAF project - "vphmi_13" to ViewPAC

2. Please plug i8024W at slot1, i8017HW at slot 2 and wire i-8024W's voltage output Ch.1 to 4 to

i-8017HW's Ch.1 to 4

Please Enter "Interval" and "Period" value and then click "Go" to start record i-8017H's Ch.1 to Ch.4
Interval (10 to 10000) milli-second :
Period (1 to 10) minute :

Operation state :
Total record number :
Current record number :
Download recore File

If recording is finished, you may click on "Download record File" to download it to your PC and save it .

0
Saving stste: