<< Web HMI Demo 8 , please download "vphmi_08" project to ViewPAC >>
Download controller's file from PC (slot 0: I-87055W)

Please switch I-8077's DI_1 or DI_2 or DI_3 to record Alarm message. And then download the file.
Communication state = 0
File's starting time =
Click on here to download Alarm.js
To delete and re-start Alarm.js in the controller You will see the file's starting time will be updated