v2.08  2018/11/05
Firmware: 1. v2.07 to v2.08
          2. upgrade firmware function which can process multiple Modbus TCP request command in one socket

Update	:  7186EL.LIB => v2.14 [2016/12/12]
	   
****************************************************************************************
v2.07  2016/07/04
Firmware: 1. v2.06 to v2.07
          2. fix bug of sending wrong UCMM connection Messge Body format.
          
Update	:  DNMXS.LIB => v3.09
          
****************************************************************************************
V2.06	 Jan-10-2014 by Alan

Firmware: 1. v2.05 to v2.06
                   2. Update XS_DNM lib v3.08(2013/05/23)=>v3.08(2013/06/04).
                       When using Set Attribute Command, the old firmware(v2.05) will send wrong CAN ID.  

****************************************************************************************

V2.05	 May-23-2013 by Andy

Firmware:  1. v2.04 to v2.05
	   2. Fix bug:
	      a. support UCMM connection Messge Body format 8/16, 16/8, 16/16
	      b. Cyclic IO communication bug

Update	:  DNMXS.LIB => v3.08

***********************************************************************************

V2.04	 Nov-07-2012 by Andy
Utility:
	   1. v2.03 to v2.04
	   2. Modify default Explicit EPR value from 250 to 1250 
	   3. Modify default IO EPR value from 200 to 1000
	   4. Add module MAC address item to "About" frame
	   5. Fix bugs:
	      a. Main frame will lost focus when using reset system function

Firmware:  1. v2.03 to v2.04
	   2. Update DNMXS.LIB: v3.06 => v3.07
	      Fix bugs:
	        a. Modify internal CAN buffer size from 5 to 35
	        b. timer bug, that will let device to send error message irregularly.
	   4. Remove Auto Search function

***********************************************************************************
V2.03	 March-03-2011 by Andy

Utility:
	   1. v2.02 to v2.03
	   2. And "Auto Start All Device" function when booting
	   3. fix bugs: 
	      a. Disable the function of getting Master status when setting module parameters

Firmware:  1. v2.02 to v2.03
	   2. add "Auto Start All Device" function and command 0x4D for this function
	   3. Mask un-used command of DNMXS library
           4. Add counterdowntimer on some function to increase DNMXS process speed
	   5. Limit the Input/Output data length to 128 bytes for each DNS device
	   6. fix bugs:
	      a. Remove invalid Clear/SetBaud function of COM port
              b. Clear Rx Software buffer when CAN Rx Data overrun
 	      c. ScanList memory size error

Update	:  DNMXS.LIB => v3.06

***********************************************************************************
V2.02   Aug-13-2010 by Andy

Utility:
	   1. v2.01 to v2.02
	   2. Modify the Utility name from "I-7243D" to "GW-7434D"

Firmware:
	   1. v2.01 to v2.02
           2. fix bugs:
	      a. Get/Set attribute ID/Class/Instance/Attribute write into wrong Modbus address
	      b. modify UpdateMBTCP_GetAttrMem(), UpdateMBTCP_SetAttrMem() 
	      c. fix Modbus_Response_Event(): after responsing a error Modbus command
		 the next command will still be error command.

Update	:  DNMXS.LIB => v3.01 

***********************************************************************************
V2.01   April-01-2010 by Andy and Johney

Firmware:
	   1. v2.00 to v2.01
	   2. fix firmware bug that reading wrong eeprom address when booting up.

Utility:
	   1. v2.00 to v2.01
	   2. modify the back color of the main frame.

***********************************************************************************
V2.00   Feb-27-2009 by Andy and Johney

Firmware:
	   1. v1.0.1 to v2.00
	   2. This version has big change with previous version.
	   3. The modbus memory address has also changed.
	   4. Add the Get / Set attbibute functions
           5. Add the Auto Search function.

Utility:
	   1. v1.0.1 to v2.00
	   2. Add Get / Set attribute functions

***********************************************************************************
v1.01	Dec-19-2008    by Andy

Firmware:
	   1. v1.0.0 to v1.0.1
	   2. Fix some bugs that will cause master stop to allocate
	      with other devices.
	   3. tcpip_dm.lib => tcp_dm32.lib
	      socket buffer 63 => 31
	   4. fix the setting NetID bug

Utility:
	   1. v1.0.0 to v1.0.1
	   2. Add EEPROM copy function via RS-232 port

Update	:  7186EL.LIB => 2007/05/08
	   tcpip_dm.lib => tcp_dm32.lib 2007/05/09
	   vl6_3223.lib => 2007/05/07
	   

