<BC>   : designed for A826PGL,use BC++ 3.1
<TC>   : designed for A826PGL,use TC 2.x 
<MSC>  : designed for A826PGL,use MSC 6.0 or latter

The driver for A826 is very similar to the one for A822. The differences
are given below:
	1 : A/D data format is different
	2 : A822_AD_PollingVar will return 0xffff if A/D timeout
	3 : A826_AD_pollingVar will also return 0xffff if A/D timeout
