/********************************************************************/
/* This document describes that how to install the A823 for LabView */
/*      This content is valid only for WINDOWS 95/98	            */
/* DATE: MAY-29, 1999						    */
/* VERSION: V02.50.01						    */
/********************************************************************/

 A). The Disk Contents:

  |--README.TXT  <-- This file.
  |
  |--\[SETUP]    <-- sub-directory
        |--Setup.exe  <-- the Setup program
      
 B). Installation Steps
    step 1). Insert 'A823 LabView for 95' disk into floppy drive(either A: or B:).
    step 2). clicking Start/Run in the task Bar
    step 3). enter the path as:
             A:\SETUP\SETUP.EXE  (if floopy drive is A:)
             B:\SETUP\SETUP.EXE  (if floopy drive is B:)
    step 4). Following those instructions in installation process 
             to complete it.

    The A823.DLL and A823.VXD will be copied into C:\WINEDOWS\SYSTEM.

 
 C). After installed, the sub-directoried tree as fillows:
    
      [Base Directory] <-- the directory you selected to setup
             |-\[DEMO]  <-- Demo Code
             |     |-\demo?.vi
             |     |-\readme.vi             
             |        
             |-\[DLL] <-- some device driver
                   |-\A823.dll    <-- dynamic linking library for A823
              	   |-\A823.VXD    <-- virtual device driver

 
              
