Demo list for £gPAC-7186EX series module

- About the detailed step that the programs compiles please refer to the Compiler.pdf.
  (CD:\NAPDOS\MiniOS7\Document\Compiler.pdf)
  (http://ftp.icpdas.com.tw/pub/cd/8000cd/napdos/minios7/document/compiler.pdf)

Folder | Demo program | Explanation
Hello | Hello_C | Detecting if the operation system is MiniOS7. Note: MSC does not support C++. Hello _ C ++ is only supported by BC.
Hello_C++
COM_Ports | C_Style_IO | 1. Shows how to write a function for input data. 2. Retrieves a string. 3. Shows how to use a C function: sscanf,or just use Scanf().
Receive | Receive COM port.
Slv_COM | The PC sends commands to the uPAC-7186EX, and receives responses from the uPAC-7186EX. Also shows how to use another COM port or LED to show information to help debug a program.
ToCom_In_Out | Reads/Writes the byte data via the COM port.
DateTime | ”@ | Reads the date and time from an RTC and prints it on a monitor (user can set the date and time).
LED | Led | Shows how to use DelayMs function to switch the LED ON or OFF.
Seg7led | Controls red led and 7-segment display.
File | Config_1_Basic | In many applications, a text file is needed in order to record specific information so that the program can read it. FSeek can be used to retrieve specific information from a text file.
Config_2_Advanced | Extends config_1_Basic, and adds GetProFileInt, GetProFileFloat, GetProFileStr. These functions can be used to determine the "Type" from a text file.
Memory | Demo5 | Read and writes to the NVRAM.
EEPROM | Writes a value to the EEPROM and shows it on the monitor.
EEPROM-r | Reads the data stored in the EEPROM.
EEPROM-w | Inputs a value and stores it in an write to EEPROM block 1 peer address (value will automatically increase by 1).
Flash | Reads, writes and erases the Flash memory.
Flash-r | Reads the value that has been written to the flash memory.
Flash-w | Inputs a value written in the flash memory (value will automatically increase by 1).
NVRAM-r | Reads the value that has been written to NVRAM.
NVRAM-w | Writes a value to the NVRAM (value will automatically increase by 1).
Top-Mem | Demonstration of the "AllocateTopMemory()" function
Misc | Reset | Restores the initial values.
Runprog | Uses Ungetch() to run another program.
SerialNumber | The serial number of the uPAC-7186EX.
Watchdog | Enables the Watchdog or bypasses the enabled Watchdog.
7K87K_Module | 7K87K_demo_for_com | Shows how to connect and control the 7k or 87k modules via COM2.
7K87K_AI_for_Com
7K87K_DI_for_Com
7K87K_DIO_for_Com
7k87K_DO_for_Com
AO_024_for_Com
AO_22_26_for_Com
Timer | Demo90 | A demonstration program showing how to use the function.
Demo91 | Shows how to use CountDownTimer function channel 0 to switch the LED ON or OFF.
Demo92 | Shows how to use StopWatch function on channel 0 to switch the led ON or OFF.
Demo96 | Shows how to use the User timer function to control the 5-digit LED.
Demo97 | Shows how to use DelayMs function to switch the LED ON or OFF.
Demo98 | Shows how to use the uPAC-7186EX timer function to send/receive data to or from 7000 series modules.
XBoard |  | These demo programs for all I/O expansion boards which are applicable to the uPAC-7186EX module.
7186FD (for 64MB flash memory on uPAC-7186EX-FD) | Utility | Utility for the MiniOS7 File System. Operations Include Dir, Read, Write, etc.
MFS_QA | Quality assurance program for the MiniOS7 File System. Including function test, read/write performance test.
Puts | How to write a string to a file in the 64MB flash memory.
Gets | How to get a string from a file in the 64MB flash memory.