Function | _SetBaudrate
Description | Sets baudrate of specific COM port of multi-serial module. This function is used for C/C++ compiler.
Function Prototype | int _SetBaudrate(int slot, int port, unsigned long baudrate)
Return | 0 : no error others : failure
slot | 0 ~ 3 for 4 slots 0 ~ 7 for 8 slots
port | 0, 1 ==> I-8112 and I-8142 0, 1, 2, 3 ==> I-8114 and I-8144
baudrate | 300,600,1200,2400,4800,9600, 19200,38400,57600,115200
Example |
Function | Ret = _SetBaudrate(0,1,9600);
Return | 0 (success)
Description | Sets the baudrate of COM1 of multi-serial module that plugged on slot0 to 9600
Reference | SetInBufSize SetOutBufSize InstallCom8000 _SetBaudrate _SetDataFormat RestoreCom8000 IsCom8000 ToCom8000 ToCom8000Str ToCom8000nBytes ReadCom8000 ReadCom8000nBytes
Modules | I-8112, I-8114, I-8142, I-8144

Back to Previous Page |