Function | IsCom8000
Description | Checks is any data in input buffer of multi-serial module. This function is used for C/C++ compiler.
Function Prototype | int IsCom8000(int slot, int port)
Return | 0 : no data in buffer 1 : some data in buffer
slot | 0 ~ 3 for 4 slots 0 ~ 7 for 8 slots
port | 0, 1 ==> I-8112 and I-8142 0, 1, 2, 3 ==> I-8114 and I-8144
Example |
Function | Ret = IsCom8000(0,1);
Return | 0 : no data in buffer 1 : some data in buffer
Description | Checks is any data in buffer of COM1 of multi-serial module that plugged on slot 0 of I-8000 MCU.
Reference | SetInBufSize SetOutBufSize InstallCom8000 _SetBaudrate _SetDataFormat RestoreCom8000 IsCom8000 ToCom8000 ToCom8000Str ToCom8000nBytes ReadCom8000 ReadCom8000nBytes
Modules | I-8112, I-8114, I-8142, I-8144

Back to Previous Page |