Function | ReadCom8000
Description | Reads one byte from specific COM port of multi-serial module. This function is used for C/C++ compiler.
Function Prototype | int ReadCom8000(int slot, int port)
Return | data value (0 ~ 255)
slot | 0 ~ 3 for 4 slots 0 ~ 7 for 8 slots
port | 0, 1 ==> I-8112 and I-8142 0, 1, 2, 3 ==> I-8114 and I-8144
Example |
Function | Data = ReadCom8000(0,1);
Return | 0x41 ('A')
Description | Reads one byte from COM1 of multi-serial module that plugged on slot 0 of I-8000 MCU.
Note | Please call IsCom800 first to confirm that there are some data in input buffer before calling this function.
Reference | SetInBufSize SetOutBufSize InstallCom8000 _SetBaudrate _SetDataFormat RestoreCom8000 IsCom8000 ToCom8000 ToCom8000Str ToCom8000nBytes ReadCom8000 ReadCom8000nBytes
Modules | I-8112, I-8114, I-8142, I-8144

Back to Previous Page |