Note:These Command Just for Master I-8000 Series(I-8410,I-8810)
Function | I8024_CurrentHexOut
Description | This function send the current HEX value to the I-8024 module in the specified channel and slot of the I-8000 system. This function is used for C/C++ compiler.
Function Prototype | void I8024_CurrentHexOut(int slot,int ch,int data)
void | Function no return
slot | Specified slot of the I-8000 system Range from 0 to 3 for 4 slot Range from 0 to 7 for 8 slot Data type : integer
ch | Output channel Range : 0 to 3 Data type : int
data | Output data with hexadecimal Data type : int data range:0h ~ 3FFFh Current Output : 0.xxx ~ +20.xxx
Note: |
Before use this function,You must use the Initial function at the first. refer to Initial Function
Example |
Function | I8024_CurrentHexOut(0,1,0x3fff)
Return | void
Description | The example send the value(0x3fff) to slot 0 of the I-8000 system.The channel 1 of I-8024 will output approximate +20.xxx mA.
Reference | I8024_VoltageOut I8024_VoltageHexOut I8024_CurrentHexOut I8024_Initial
Modules | I-8024

Back to Previous Page |