2:16:57 PM-> English
2:16:57 PM-> Chinese
2:16:57 PM-> Don't show this next time
2:16:57 PM-> Search RU-87PN Addr. Mode
2:16:57 PM-> Modbus Editor
2:16:57 PM-> COM Port
2:16:57 PM-> Start Search
2:16:57 PM-> Stop Search
2:16:57 PM-> Command Line
2:16:57 PM-> Remote I/O quick configuration
2:16:57 PM-> CE/WES Backup/Restore backplane I-87K I/O configurations
2:16:57 PM-> Offline Configuration for 87PN
2:16:57 PM-> Data Logger
2:16:57 PM-> Language
2:16:57 PM-> FAQ
2:16:57 PM-> End Address
2:16:57 PM-> Start Address
2:16:57 PM-> ID
2:16:57 PM-> Address
2:16:57 PM-> Baud Rate
2:16:57 PM-> Checksum
2:16:57 PM-> Format
2:16:57 PM-> Status
2:16:57 PM-> Description
2:16:57 PM-> COM:1
2:17:22 PM-> 01H
2:17:22 PM-> 7
2:17:22 PM-> RF Channel
2:17:22 PM-> RF Pan ID
2:17:22 PM-> Reverse DO State
2:17:22 PM-> ms
2:17:22 PM-> Min. Half Pulse Width
2:17:22 PM-> RF Power
2:17:22 PM-> Enable ZT Software Configuration
2:17:22 PM-> 1
2:17:22 PM-> Response Delay
2:17:22 PM-> Parity
2:17:22 PM-> Checksum
2:17:22 PM-> Baud Rate
2:17:22 PM-> Protocol
2:17:22 PM-> Address
2:17:22 PM-> 01H
2:17:22 PM-> 7
2:17:22 PM-> RF Channel
2:17:22 PM-> RF Pan ID
2:17:22 PM-> Reverse DO State
2:17:22 PM-> ms
2:17:22 PM-> Min. Half Pulse Width
2:17:22 PM-> RF Power
2:17:22 PM-> Enable ZT Software Configuration
2:17:22 PM-> 1
2:17:22 PM-> Response Delay
2:17:22 PM-> Parity
2:17:22 PM-> Checksum
2:17:22 PM-> Baud Rate
2:17:22 PM-> Protocol
2:17:22 PM-> Address
2:17:22 PM-> Type Code
2:17:22 PM-> AI Value
2:17:22 PM-> Set all channels as CH0
2:17:22 PM-> Sample Rate
2:17:22 PM-> CH:00
2:17:22 PM-> CH:0
2:17:22 PM-> CH:01
2:17:22 PM-> CH:1
2:17:22 PM-> CH:02
2:17:22 PM-> CH:2
2:17:22 PM-> CH:03
2:17:22 PM-> CH:3
2:17:22 PM-> 01H
2:17:22 PM-> 7
2:17:22 PM-> RF Channel
2:17:22 PM-> RF Pan ID
2:17:22 PM-> Reverse DO State
2:17:22 PM-> ms
2:17:22 PM-> Min. Half Pulse Width
2:17:22 PM-> RF Power
2:17:22 PM-> Enable ZT Software Configuration
2:17:22 PM-> 1
2:17:22 PM-> Response Delay
2:17:22 PM-> Parity
2:17:22 PM-> Checksum
2:17:22 PM-> Baud Rate
2:17:22 PM-> Protocol
2:17:22 PM-> Address
2:17:22 PM-> Type Code
2:17:22 PM-> AI Value
2:17:22 PM-> Set all channels as CH0
2:17:22 PM-> Sample Rate
2:17:22 PM-> CH:00
2:17:22 PM-> CH:0
2:17:22 PM-> CH:01
2:17:22 PM-> CH:1
2:17:22 PM-> CH:02
2:17:22 PM-> CH:2
2:17:22 PM-> CH:03
2:17:22 PM-> CH:3
2:17:22 PM-> WDT Timeout Count
2:17:22 PM-> Enable Output When WDT Timeout
2:17:22 PM-> Set Timer
2:17:22 PM-> (0.1 ~ 25.5 sec)
2:17:22 PM-> Reset Watchdog Status
2:17:22 PM-> Auto Send Host OK
2:17:22 PM-> Enable WDT
2:17:22 PM-> WDT Timeout
2:17:22 PM-> 01H
2:17:22 PM-> 7
2:17:22 PM-> RF Channel
2:17:22 PM-> RF Pan ID
2:17:22 PM-> Reverse DO State
2:17:22 PM-> ms
2:17:22 PM-> Min. Half Pulse Width
2:17:22 PM-> RF Power
2:17:22 PM-> Enable ZT Software Configuration
2:17:22 PM-> 1
2:17:22 PM-> Response Delay
2:17:22 PM-> Parity
2:17:22 PM-> Checksum
2:17:22 PM-> Baud Rate
2:17:22 PM-> Protocol
2:17:22 PM-> Address
2:17:22 PM-> Type Code
2:17:22 PM-> AI Value
2:17:22 PM-> Set all channels as CH0
2:17:22 PM-> Sample Rate
2:17:22 PM-> CH:00
2:17:22 PM-> CH:0
2:17:22 PM-> CH:01
2:17:22 PM-> CH:1
2:17:22 PM-> CH:02
2:17:22 PM-> CH:2
2:17:22 PM-> CH:03
2:17:22 PM-> CH:3
2:17:22 PM-> WDT Timeout Count
2:17:22 PM-> Enable Output When WDT Timeout
2:17:22 PM-> Set Timer
2:17:22 PM-> (0.1 ~ 25.5 sec)
2:17:22 PM-> Reset Watchdog Status
2:17:22 PM-> Auto Send Host OK
2:17:22 PM-> Enable WDT
2:17:22 PM-> WDT Timeout
2:17:22 PM-> Reverse DI State  (INIT*)
2:17:22 PM-> DI Bit Status
2:17:22 PM-> 0
2:17:22 PM-> DI Value
2:17:22 PM-> 01H
2:17:22 PM-> 7
2:17:22 PM-> RF Channel
2:17:22 PM-> RF Pan ID
2:17:22 PM-> Reverse DO State
2:17:22 PM-> ms
2:17:22 PM-> Min. Half Pulse Width
2:17:22 PM-> RF Power
2:17:22 PM-> Enable ZT Software Configuration
2:17:22 PM-> 1
2:17:22 PM-> Response Delay
2:17:22 PM-> Parity
2:17:22 PM-> Checksum
2:17:22 PM-> Baud Rate
2:17:22 PM-> Protocol
2:17:22 PM-> Address
2:17:22 PM-> Type Code
2:17:22 PM-> AI Value
2:17:22 PM-> Set all channels as CH0
2:17:22 PM-> Sample Rate
2:17:22 PM-> CH:00
2:17:22 PM-> CH:0
2:17:22 PM-> CH:01
2:17:22 PM-> CH:1
2:17:22 PM-> CH:02
2:17:22 PM-> CH:2
2:17:22 PM-> CH:03
2:17:22 PM-> CH:3
2:17:22 PM-> WDT Timeout Count
2:17:22 PM-> Enable Output When WDT Timeout
2:17:22 PM-> Set Timer
2:17:22 PM-> (0.1 ~ 25.5 sec)
2:17:22 PM-> Reset Watchdog Status
2:17:22 PM-> Auto Send Host OK
2:17:22 PM-> Enable WDT
2:17:22 PM-> WDT Timeout
2:17:22 PM-> Reverse DI State  (INIT*)
2:17:22 PM-> DI Bit Status
2:17:22 PM-> 0
2:17:22 PM-> DI Value
2:17:22 PM-> Low Latch
2:17:22 PM-> High Latch
2:17:22 PM-> Clear DI Latch
2:17:22 PM-> 01H
2:17:22 PM-> 7
2:17:22 PM-> RF Channel
2:17:22 PM-> RF Pan ID
2:17:22 PM-> Reverse DO State
2:17:22 PM-> ms
2:17:22 PM-> Min. Half Pulse Width
2:17:22 PM-> RF Power
2:17:22 PM-> Enable ZT Software Configuration
2:17:22 PM-> 1
2:17:22 PM-> Response Delay
2:17:22 PM-> Parity
2:17:22 PM-> Checksum
2:17:22 PM-> Baud Rate
2:17:22 PM-> Protocol
2:17:22 PM-> Address
2:17:22 PM-> Type Code
2:17:22 PM-> AI Value
2:17:22 PM-> Set all channels as CH0
2:17:22 PM-> Sample Rate
2:17:22 PM-> CH:00
2:17:22 PM-> CH:0
2:17:22 PM-> CH:01
2:17:22 PM-> CH:1
2:17:22 PM-> CH:02
2:17:22 PM-> CH:2
2:17:22 PM-> CH:03
2:17:22 PM-> CH:3
2:17:22 PM-> WDT Timeout Count
2:17:22 PM-> Enable Output When WDT Timeout
2:17:22 PM-> Set Timer
2:17:22 PM-> (0.1 ~ 25.5 sec)
2:17:22 PM-> Reset Watchdog Status
2:17:22 PM-> Auto Send Host OK
2:17:22 PM-> Enable WDT
2:17:22 PM-> WDT Timeout
2:17:22 PM-> Reverse DI State  (INIT*)
2:17:22 PM-> DI Bit Status
2:17:22 PM-> 0
2:17:22 PM-> DI Value
2:17:22 PM-> Low Latch
2:17:22 PM-> High Latch
2:17:22 PM-> Clear DI Latch
2:17:22 PM-> DI Counter
2:17:22 PM-> CH: 00
2:17:22 PM-> Clear
2:17:22 PM-> CH: 01
2:17:23 PM-> 01H
2:17:23 PM-> 7
2:17:23 PM-> RF Channel
2:17:23 PM-> RF Pan ID
2:17:23 PM-> Reverse DO State
2:17:23 PM-> ms
2:17:23 PM-> Min. Half Pulse Width
2:17:23 PM-> RF Power
2:17:23 PM-> Enable ZT Software Configuration
2:17:23 PM-> 1
2:17:23 PM-> Response Delay
2:17:23 PM-> Parity
2:17:23 PM-> Checksum
2:17:23 PM-> Baud Rate
2:17:23 PM-> Protocol
2:17:23 PM-> Address
2:17:23 PM-> Type Code
2:17:23 PM-> AI Value
2:17:23 PM-> Set all channels as CH0
2:17:23 PM-> Sample Rate
2:17:23 PM-> CH:00
2:17:23 PM-> CH:0
2:17:23 PM-> CH:01
2:17:23 PM-> CH:1
2:17:23 PM-> CH:02
2:17:23 PM-> CH:2
2:17:23 PM-> CH:03
2:17:23 PM-> CH:3
2:17:23 PM-> WDT Timeout Count
2:17:23 PM-> Enable Output When WDT Timeout
2:17:23 PM-> Set Timer
2:17:23 PM-> (0.1 ~ 25.5 sec)
2:17:23 PM-> Reset Watchdog Status
2:17:23 PM-> Auto Send Host OK
2:17:23 PM-> Enable WDT
2:17:23 PM-> WDT Timeout
2:17:23 PM-> Reverse DI State  (INIT*)
2:17:23 PM-> DI Bit Status
2:17:23 PM-> 0
2:17:23 PM-> DI Value
2:17:23 PM-> Low Latch
2:17:23 PM-> High Latch
2:17:23 PM-> Clear DI Latch
2:17:23 PM-> DI Counter
2:17:23 PM-> CH: 00
2:17:23 PM-> Clear
2:17:23 PM-> CH: 01
2:17:23 PM-> Alarm Mode
2:17:23 PM-> Low Alarm Limit
2:17:23 PM-> High Alarm Limit
2:17:23 PM-> Set Alarm
2:17:23 PM-> 01H
2:17:23 PM-> 7
2:17:23 PM-> RF Channel
2:17:23 PM-> RF Pan ID
2:17:23 PM-> Reverse DO State
2:17:23 PM-> ms
2:17:23 PM-> Min. Half Pulse Width
2:17:23 PM-> RF Power
2:17:23 PM-> Enable ZT Software Configuration
2:17:23 PM-> 1
2:17:23 PM-> Response Delay
2:17:23 PM-> Parity
2:17:23 PM-> Checksum
2:17:23 PM-> Baud Rate
2:17:23 PM-> Protocol
2:17:23 PM-> Address
2:17:23 PM-> Type Code
2:17:23 PM-> AI Value
2:17:23 PM-> Set all channels as CH0
2:17:23 PM-> Sample Rate
2:17:23 PM-> CH:00
2:17:23 PM-> CH:0
2:17:23 PM-> CH:01
2:17:23 PM-> CH:1
2:17:23 PM-> CH:02
2:17:23 PM-> CH:2
2:17:23 PM-> CH:03
2:17:23 PM-> CH:3
2:17:23 PM-> WDT Timeout Count
2:17:23 PM-> Enable Output When WDT Timeout
2:17:23 PM-> Set Timer
2:17:23 PM-> (0.1 ~ 25.5 sec)
2:17:23 PM-> Reset Watchdog Status
2:17:23 PM-> Auto Send Host OK
2:17:23 PM-> Enable WDT
2:17:23 PM-> WDT Timeout
2:17:23 PM-> Reverse DI State  (INIT*)
2:17:23 PM-> DI Bit Status
2:17:23 PM-> 0
2:17:23 PM-> DI Value
2:17:23 PM-> Low Latch
2:17:23 PM-> High Latch
2:17:23 PM-> Clear DI Latch
2:17:23 PM-> DI Counter
2:17:23 PM-> CH: 00
2:17:23 PM-> Clear
2:17:23 PM-> CH: 01
2:17:23 PM-> Alarm Mode
2:17:23 PM-> Low Alarm Limit
2:17:23 PM-> High Alarm Limit
2:17:23 PM-> Set Alarm
2:17:23 PM-> Low Alarm Status
2:17:23 PM-> High Alarm Status
2:17:23 PM-> DO Bit Status
2:17:23 PM-> Read Safe Value
2:17:23 PM-> Read Power On Value
2:17:23 PM-> Read DO
2:17:23 PM-> Set to [Safe Value]
2:17:23 PM-> Set to [Power On Value]
2:17:23 PM-> DO0
2:17:23 PM-> DO1
2:17:23 PM-> 01H
2:17:23 PM-> 7
2:17:23 PM-> RF Channel
2:17:23 PM-> RF Pan ID
2:17:23 PM-> Reverse DO State
2:17:23 PM-> ms
2:17:23 PM-> Min. Half Pulse Width
2:17:23 PM-> RF Power
2:17:23 PM-> Enable ZT Software Configuration
2:17:23 PM-> 1
2:17:23 PM-> Response Delay
2:17:23 PM-> Parity
2:17:23 PM-> Checksum
2:17:23 PM-> Baud Rate
2:17:23 PM-> Protocol
2:17:23 PM-> Address
2:17:23 PM-> Type Code
2:17:23 PM-> AI Value
2:17:23 PM-> Set all channels as CH0
2:17:23 PM-> Sample Rate
2:17:23 PM-> CH:00
2:17:23 PM-> CH:0
2:17:23 PM-> CH:01
2:17:23 PM-> CH:1
2:17:23 PM-> CH:02
2:17:23 PM-> CH:2
2:17:23 PM-> CH:03
2:17:23 PM-> CH:3
2:17:23 PM-> WDT Timeout Count
2:17:23 PM-> Enable Output When WDT Timeout
2:17:23 PM-> Set Timer
2:17:23 PM-> (0.1 ~ 25.5 sec)
2:17:23 PM-> Reset Watchdog Status
2:17:23 PM-> Auto Send Host OK
2:17:23 PM-> Enable WDT
2:17:23 PM-> WDT Timeout
2:17:23 PM-> Reverse DI State  (INIT*)
2:17:23 PM-> DI Bit Status
2:17:23 PM-> 0
2:17:23 PM-> DI Value
2:17:23 PM-> Low Latch
2:17:23 PM-> High Latch
2:17:23 PM-> Clear DI Latch
2:17:23 PM-> DI Counter
2:17:23 PM-> CH: 00
2:17:23 PM-> Clear
2:17:23 PM-> CH: 01
2:17:23 PM-> Alarm Mode
2:17:23 PM-> Low Alarm Limit
2:17:23 PM-> High Alarm Limit
2:17:23 PM-> Set Alarm
2:17:23 PM-> Low Alarm Status
2:17:23 PM-> High Alarm Status
2:17:23 PM-> DO Bit Status
2:17:23 PM-> Read Safe Value
2:17:23 PM-> Read Power On Value
2:17:23 PM-> Read DO
2:17:23 PM-> Set to [Safe Value]
2:17:23 PM-> Set to [Power On Value]
2:17:23 PM-> DO0
2:17:23 PM-> DO1
2:17:23 PM-> Configuration
2:17:23 PM-> DSub Connector
2:17:23 PM-> Set Module Configurations
2:17:23 PM-> Enable Check Command Received Timeout
2:17:23 PM-> Analog Format
2:17:23 PM-> Sample Mode
2:17:23 PM-> 60/50 Hz
2:17:23 PM-> AI/DO Alarm
2:17:23 PM-> SingleEnd
2:17:23 PM-> Enable SingleEnded
2:17:23 PM-> DI
2:17:23 PM-> Host WDT
2:17:23 PM-> Commands Log
2:17:23 PM-> Export Commands
2:17:23 PM-> Log All Commands
2:17:23 PM-> Save to path\log_report\
2:17:23 PM-> About
2:17:23 PM-> Exit
