Function | ToCom8000Str
Description | Sends a string to specific COM port of multi-serial module. This function is used for C/C++ compiler.
Function Prototype | int ToCom8000Str(int slot, int port, char *str)
Return | 0 : success other : failure
slot | 0 ~ 3 for 4 slots 0 ~ 7 for 8 slots
port | 0, 1 ==> I-8112 and I-8142 0, 1, 2, 3 ==> I-8114 and I-8144
*str | pointer to indicate the output string
Example |
Function | Ret = ToCom8000Str(0,1,Str);
Return | 0 (success)
Description | Sends string, Str, to COM1 of multi-serial module that plugged on slot 0 of I-8000 MCU.
Reference | SetInBufSize SetOutBufSize InstallCom8000 _SetBaudrate _SetDataFormat RestoreCom8000 IsCom8000 ToCom8000 ToCom8000Str ToCom8000nBytes ReadCom8000 ReadCom8000nBytes
Modules | I-8112, I-8114, I-8142, I-8144

Back to Previous Page |