
                                     DIO-64
   
        ** 32 DIGITAL INPUT & 32 DIGITAL OUTPUT WITH TIMER / COUNTER **

=============================================================================




Demo program list

DEMO_01.EXE ------> Digital input / output demo program
IRQ_TIM.EXE ------> Interrupt timer trigger demo program
IRQ_EVNT.EXE -----> Interrupt Event trigger demo program
COUNTER.EXE ------> Timer/Counter demo program


I/O address : 0x2A0      SW1 : off on  off on  off on  
                                1   2   3   4   5   6
IRQ level : 5

-----------------------------------------------------------------------------

Note :

1. Interrupt timer trigger mode & event trigger mode neet second 8254 chip.
    (DIO-64/6 only)

2. The second 8254 chip is option item

Ordering information :

          DIO-64/3 :  32 digital input & 32 digital output 
                      with One 8254 ( three 16 bit Counter )

          DIO-64/6 :  32 digital input & 32 digital output
                      with Two 8254 
                      ( Four 16 bit counter & One 32 bit counter ) 
                      
                      Note : 32 bit counter is cascaded (Counter 4,5)

          DB-16P  :   16 channel OPTO-isolated terminal board
          
          DB-16R  :   16 channel relay output termainal board 
          
          NAPWIN  :   for Windows 95 driver

          NAPWNT  :   for Windows NT driver

          NAPVIEW :   for LabVIEW driver



                                                           ICP DAS 02.20.97 
============================================================================
