/**************************************************************/
/*                                                            */
/*  ISO-AD32 Development Toolkit                              */
/*  for Windows NT/2000                                       */
/*                                                            */
/*  Version : v2.21.00                                        */
/*  Date    : Feb-08-2001                                     */
/*                                                            */
/*  For Windows NT/2000 User to install the ISO-AD32 Toolkit  */
/**************************************************************/

The READNE.TXT contains the newset information for ISOAD32.
Please reading this file before install.

A). The Disk Contents:

    If you download the toolkit from our web, please...
      A-1. Create an temp folder, for example: "c:\setup".
      A-2. Run the Disk1.exe to extract the setup programs to
           the temp folder, for example: "c:\setup".
           ( Disk1.exe is an self-extraction file )
      A-3. Copy the related Data?.cab into the temp folder.
           (for example: "c:\setup".)

    If you have the CD-ROM with the board, please refer to the 
    "Readme.txt" file (under the root folder of CD-ROM) to find 
    out the folder that contains the related toolkit .


    |--\README.TXT       <-- This file.
    |
    |--\SETUP            <-- sub-directory
        |--\Setup.exe    <-- the Setup program


B). Installation Steps

    B-1. Insert disc into CD-ROM drive ( D: or ... ).
    B-2. clicking Start/Run in the task Bar.
    B-3. enter the path and file name to run it. 
         (Install from the CD-ROM or the temp folder that you 
          download and save the files into.)

    (Note: You also can follows the MENU to install the software
           if your system supports Auto-Run mechanism.)

    B-4. Following those instructions in installation process 
         to complete it.

    B-5. Shutdown your system.
    B-6. Plug the data-acquisition board into your system.
    B-7. Start your system.



C). After installed,

     The AD32.DLL will be copied into C:\WINNT\SYSTEM32 
     The NAPWNT.SYS will be copied into C:\WINNT\SYSTEM32\DRIVERS
 

     Following registry key and value will be created ......
     HKEY_LOCAL_MACHINE:
	 system\CurrentControlSet\Services\Napwnt\ErrorControl=0x00000001
	 system\CurrentControlSet\Services\Napwnt\Start=0x00000002
	 system\CurrentControlSet\Services\Napwnt\Type=0x00000001

    
     The item "DAQPro ISOAD32 NT" will be added 
     into the "Add/Remove Programs" (under "Control Panel") 


D). After installing, the directories as follows:

     The default [Base Directory] is "\DAQPro\ISOAD32_NT".

     [Base Directory] <-- the directory you selected to setup
        |--\DEMO
        |  |--\VB5             <-- VB 5.0 sample code
        |  |  |--\AD           <-- AD Demo
        |  |  +--\ADScan       <-- AD Demo (with Channel-Scan)
        |  |
        |  |--\VC5             <-- Visual C++ sample code  
        |  |  |--\AD           <-- AD Demo
        |  |  +--\ADScan       <-- AD Demo (with Channel-Scan)
        |  |
	|  |--\Delphi3         <-- Delphi 3.0 sample code	
        |  |  |--\AD           <-- AD Demo
        |  |  |--\ADScan       <-- AD Demo (with Channel-Scan)
        |  |  +--\Diag         <-- Diagnostic Program
        |  |
	|  +--\BCB3            <-- Borland C++ Builder 3.0 sample code
        |     |--\AD           <-- AD Demo
        |     +--\ADScan       <-- AD Demo (with Channel-Scan)
	|
        |--\Manual
	|  |--\AD32soft.pdf    <-- Software manual
	|  |--\AD32hard.pdf    <-- Hardware manual
        |  |--\CallDLL.pdf     <-- Call the DLL functions 
        |  |                       with VC++5.0, VB5.0, Delphi3.0 
        |  |                       and Borland C++ Builder 3.0.
        |  +--\ResCheck.pdf    <-- Check the resoures 
        |                           under Windows 95/98/NT
	|
	|--\Diag
	|  +--\Diag.exe        <-- Diagnostic program
	|
        |--\Driver
        |  |--\AD32.DLL   	<-- Dynamic Linking Library
	|  |--\Napwnt.sys  	<-- device driver	
        |  |
        |  |--\BCB3            <-- for Borland C++ Builder 3
        |  |  |--\AD32.h       <-- Header file
        |  |  +--\AD32.Lib     <-- Import Library for BCB only
        |  |   
        |  |--\Delphi3         <-- for Delphi 3
        |  |  +--\AD32.pas     <-- Declaration file
        |  |   
        |  |--\VB5             <-- for Visual Basic 5
        |  |  +--\AD32.bas     <-- Declaration file
        |  |   
        |  +--\VC5             <-- for Visual C++ 5
        |     |--\AD32.h       <-- Header file
        |     +--\AD32.Lib     <-- Import Library for VC only
	|
	|--\WhatNew.Txt         <-- What's New
	+--\Readme.Txt		<-- this file

 E). After installed, the following links will be add into the "Start Menu".
    
   [Start]    <-- the Start menu
    |--\Programs
        |--\DAQPro     
            |--\ISOAD32 NT               <-- link to the "ISOAD32_NT" folder
            |--\ISOAD32 NT - Diagnostic  <-- link to the Diagnostic Program


Note: The manual is written in PDF format,
      the user may need to free download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html 

