/************************************************************************/
/*                                                                      */
/*  ISO-813 Development Toolkit                                         */
/*  for Windows 95/98                                                   */
/*                                                                      */
/*                                                                      */
/*  Version : v1.10.30                                                  */
/*  Date    : Nov-20-1999                                               */
/*                                                                      */
/*                                                                      */
/*  For WINDOWS 95/98 User to install the ISO-813 Development Toolkit   */
/************************************************************************/

The READNE.TXT contains the newset information for ISO-813.
Please reading this file before install.

 A). The contents in this disk are valid for ISO-813.

 

 B). to run 

	  A:\SETUP\SETUP.EXE 
     or   [DriveLetter]:[\SetupProgramPath]\SETUP.EXE 

     to install the Toolkit for ISO-813.
     (please enter the path according to your environment)



 C). After installed, 

     the Iso813.dll and Napdio.vxd
     will be copied into C:\Windows\SYSTEM 

     The item "DAQPro ISO813 Win95" will be added 
     into the "Add/Remove Programs" (under "Control Panel") 
 


 D). After installing, the directories as follows:

     The default [Base Directory] is "\DAQPro\ISO813 Win95".
 
     [Base Directory] <-- the directory you selected to setup
	|--\DEMO
        |   |--\VB5     	<-- VB 5.0 sample code
        |   |--\VC5     	<-- Visual C++ sample code  
	|   |--\Delphi3     	<-- Delphi 3.0 sample code	
	|   +--\BCB3	      	<-- Borland C++ Builder 3.0 sample code
	|
	|--\Diag
	|   +--\Diag.exe        <-- Diagnostic program   
	|
        |--\Manual
	|   |--\I813soft.pdf    <-- software manual for ISO-813
	|   |--\I813hard.pdf    <-- hardware manual for ISO-813
        |   |--\CallDLL.pdf     <-- Call the DLL functions 
        |   |                       with VC++5.0, VB5.0, Delphi3.0 
        |   |                       and Borland C++ Builder 3.0.
        |   |--\ResCheck.pdf    <-- Check the resoures 
        |   |                       under Windows 95/98/NT
        |   +--\SoftInst.pdf    <-- user's manual for software installation         
	|
	|--\Driver
        |   |--\ISO813.DLL   	<-- Dynamic Linking Library
	|   |--\Napdio.Vxd  	<-- device driver	
	|   |--\BC
	|   |   |--\Iso813.h    <-- Header file
	|   |   +--\Iso813.lib  <-- Import Library for BCB
	|   |   
	|   |--\Delphi
	|   |   +--\Iso813.pas  <-- Declaration file
	|   |   
	|   |--\VB
	|   |   +--\Iso813.pas  <-- Declaration file
	|   |   
	|   +--\VC
	|       |--\Iso813.h    <-- Header file
	|       +--\Iso813.lib  <-- Import Library for VC++
	|
	|--\WhatNew.txt         <-- What's New
	+--\Readme.Txt		<-- this file

        

 E). After installed, the following links will be add into the "Start Menu".
    
     [Start]    <-- the Start menu
      |--\Programs
          |--\DAQPro     
              |--\ISO813 Win95               <-- link to the "ISO813 Win95" folder
              +--\ISO813 Win95 - Diagnostic  <-- link to the Diagnostic Program


*********************************************
Errata :
  On the page 12 of the Hardware Manual.
  The JP2 setting to Unipolar and JP1 setting to 20V; 
  Error : 
     the input range:  Not use, 0~10v,   0~5v,    0~2.5v,  0~1.25v
  Correct : 
     the input range:  Not use, Not use, Not use, Not use, Not use


*********************************************


Note: The manual is written in PDF format,
      the user may need to free download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html 

 		