/**************************************************************/
/*                                                            */
/*  Servo300 Development Toolkit                              */
/*  for Windows NT/2000                                       */
/*                                                            */
/*  Version : v2.00.00                                        */
/*  Date    : May-11-2001                                     */
/*                                                            */
/*  For Windows NT/2000 User to install the Servo300 Toolkit  */
/**************************************************************/

The READNE.TXT contains the newset information for Servo300.
Please reading this file before install.

A). The Disk Contents:

    If you download the toolkit from our web, please...
      A-1. Create an temp folder, for example: "c:\setup".
      A-2. Run the Disk1.exe to extract the setup programs to
           the temp folder, for example: "c:\setup".
           ( Disk1.exe is an self-extraction file )
      A-3. Copy the related Data?.cab into the temp folder.
           (for example: "c:\setup".)

    If you have the CD-ROM with the board, please refer to the 
    "Readme.txt" file (under the root folder of CD-ROM) to find 
    out the folder that contains the related toolkit .


    |--\README.TXT       <-- This file.
    |
    |--\SETUP            <-- sub-directory
        |--\Setup.exe    <-- the Setup program


B). Installation Steps

    B-1. Insert disc into CD-ROM drive ( D: or ... ).
    B-2. clicking Start/Run in the task Bar.
    B-3. enter the path and file name to run it. 
         (Install from the CD-ROM or the temp folder that you 
          download and save the files into.)

    (Note: You also can follows the MENU to install the software
           if your system supports Auto-Run mechanism.)

    B-4. Following those instructions in installation process 
         to complete it.

    B-5. Shutdown your system.
    B-6. Plug the data-acquisition board into your system.
    B-7. Start your system.



 C). After installed,

     The Servo32.dll will be copied into C:\WINNT\SYSTEM32 
     The Napwnt.sys will be copied into C:\WINNT\SYSTEM32\DRIVERS
 

     Following registry key and value will be created ......
     HKEY_LOCAL_MACHINE:
	 system\CurrentControlSet\Services\Napwnt\ErrorControl=0x00000001
	 system\CurrentControlSet\Services\Napwnt\Start=0x00000002
	 system\CurrentControlSet\Services\Napwnt\Type=0x00000001

     
     The item "DAQPro Servo300 NT" will be added 
     into the "Add/Remove Programs" (under "Control Panel") 


 D). After installed, the directories as follows:

     The default [Base Directory] is "\DAQPro\Servo300_NT".

     [Base Directory] <-- the directory you selected to setup
	|--\DEMO
        |   |--\VB5     	  <-- VB 5.0 sample code
	|   |--\Delphi3     	  <-- Delphi 3.0 sample code	
	|   +--\BCB3	       	  <-- Borland C++ Builder 3.0 sample code
	|
        |--\Manual
	|   |--\Sv3.pdf  	  <-- the hardware manual for Servo300
        |   |--\CallDLL.pdf       <-- describes how to call the DLL functions 
        |   |                         with VC++5.0, VB5.0, Delphi3.0 
        |   |                         and Borland C++ Builder 3.0.
        |   +--\ResCheck.pdf      <-- describes how to check the resoures 
        |                             under Windows 95/98/NT/2000
	|
	|--\Driver
        |   |--\Servo32.DLL   	  <-- Dynamic Linking Library
	|   |--\Napwnt.sys  	  <-- device driver	
        |   |
        |   |--\VC5               <-- for Visual C++ 5
        |   |   |--\Servo32.h     <-- Header file
        |   |   +--\Servo32.Lib   <-- Import Library for VC only
        |   |--\VB5               <-- for Visual Basic 5 
        |   |   +--\Servo32.bas   <-- Declaration file
        |   |--\Delphi3           <-- for Delphi 3
        |   |   +--\Servo32.pas   <-- Declaration file
        |   +--\BCB3              <-- for Borland C++ Builder 3
        |       |--\Servo32.h     <-- Header file
        |       +--\BCServo32.Lib <-- Import Library for BCB only
	|
	+--\Readme.Txt	          <-- this file

 E). After installed, the following links will be add into the "Start Menu".
    
   [Start]    <-- the Start menu
    |--\Programs
        |--\DAQPro     
            |--\Servo300 NT            <-- link to the "Servo300_NT" folder
                         


Note: The manual is written in PDF format,
      the user may need to free download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html 

 		