Note:These Command Just for Master I-8000 Series(I-8410,I-8810)
Function | I8024_Initial
Description | This function initialize the I-8024 module in the specified slot of the I-8000 system. This function is used for C/C++ compiler.
Function Prototype | void I8024_Initial(int slot)
void | Function no return
slot | Specified slot of the I-8000 system Range from 0 to 3 for 4 slot Range from 0 to 7 for 8 slot Data type : integer
Note: |
Before use the other function,You must use the Initial function at the first.
Example |
Function | I8024_Initial(0)
Return | void
Description | The example initial the I-8024 Module in the slot 0 of the I-8000 system.
Reference | I8024_VoltageOut I8024_VoltageHexOut I8024_CurrentOut I8024_CurrentHexOut
Modules | I-8024

Back to Previous Page |