Function | RestoreCom8000
Description | Restores multi-serial module. If you won't use the multi-serial module any more, you should call this function to release resource. This function is used for C/C++ compiler.
Function Prototype | int RestoreCom8000(int slot)
Return | 0 : no error other : restore failure
slot | 0 ~ 3 for 4 slots 0 ~ 7 for 8 slots
Example |
Function | Ret=RestoreCom8000(int slot);
Return | 0 ( success) other : failure
Description | Restores multi-serial module that plugged on slot 0 of I-8000 MCU.
Reference | SetInBufSize SetOutBufSize InstallCom8000 _SetBaudrate _SetDataFormat RestoreCom8000 IsCom8000 ToCom8000 ToCom8000Str ToCom8000nBytes ReadCom8000 ReadCom8000nBytes
Modules | I-8112, I-8114, I-8142, I-8144

Back to Previous Page |