Function | SetInBufSize
Description | Sets input buffer size for every COM ports of specific multi-serial module. Default buffer size is 1024 bytes. After calling this function, you must call InstallCom8000 to effect this setting. This function is used for C/C++ compiler.
Function Prototype | int SetInBufSize(int size)
Return | 0 : no error other : failure
size | 1 ~ 32767 (byte)
Example |
Function | Ret=SetInBufSize(2048);
Return | 0 ( success)
Description | Sets input buffer size of multi-serial module to 2048 bytes.
Note | All COM ports of same multi-serial module use same input buffer size.
Reference | SetInBufSize SetOutBufSize InstallCom8000 _SetBaudrate _SetDataFormat RestoreCom8000 IsCom8000 ToCom8000 ToCom8000Str ToCom8000nBytes ReadCom8000 ReadCom8000nBytes
Modules | I-8112, I-8114, I-8142, I-8144

Back to Previous Page |