Functions --> Demos mapping list.

Demo --> Function mapping list

Function for 7188e & 8000 | Xserver demos
64 bits unique hardware serial number | Demo19
7-Seg LED | Demo14, Demo21
COM port | Demo7, Demo15, Demo16, Demo18, Demo22
Connect 7000 Modules | Demo15, Demo18, Demo22, Demo32, Demo45
Connect 87k Modules | Demo33, Demo46,
Data Acquisition & Compression & Averaging | Demo22, Demo25
EEPROM |
Flash memory |
File in Flash (Support read file information) | Demo28, Demo29¡@
I/O (for expansion boards or 7188EA) | Demo6, Demo11, Demo13, Demo17, Demo28
NVRAM | Demo20
Original Xserver | Demo4, Demo5, Demo9, Demo12,Demo23
RTC (Real Time Clock) |
Stdio & Misc | Demo8
Timer |
Timer count down | Demo24
VcomSendSocket | Demo23, Demo37
WDT (Watch Dog Timer) | Demo10

Function for 8000 only | Xserver demos
ChangeToSlot | Demo36, Demo46, Demo49
SetA10 SetA12 SetB1A5 SetB1A6 |
GetNetId | Demo46
ModuleType NameOfModule | Demo36, Demo49
ShowLED8 ShowLED16 | Demo38
GetNumberOfSlot | Demo36, Demo46, Demo49
I/O (for 8000 modules) | Demo40, Demo41, Demo42, Demo43, Demo44, Demo49
SetLedL1, SetLedL2, SetLedL3 | Demo39
ClrSlotInt |
GetSlotInt |
IsSystemKey | Demo37
GetSystemKey | Demo37
ClearSystemKey |

Note:
For more Xserver demo programs on iPAC-8441/8841 , they are located at
http://ftp.icpdas.com/pub/cd/8000cd/napdos/8000/843x883x/tcp/xserver/demo/bc/
The demos must compile with the iPAC-8000 lib at
http://ftp.icpdas.com/pub/cd/8000cd/napdos/ipac8000/demo/tcp_demo/xserver/lib

About MiniOS7 document and API function , please refer to http://ftp.icpdas.com/pub/cd/8000cd/napdos/minios7/document/